#### Step 1: Configure PC-DMIS

Verify PC-DMIS's setup, and check if the standard settings in PC-DMIS correspond to ChorusNT settings. For example verify the CMM axis conventions and probe head Orientation and Top Speed (CMM max move speed) value.

Use Settings Editor to set the following options in the DMIS section:

- DMISMaxMeasurementVelocityMMPS = maximum measure speed

- DMISFedratPcntOfMaxMachineSpeed = 0