### Zeiss Interface

The Zeiss interface is used with manual Zeiss machines.

Before starting PC-DMIS, rename the Zeiss.dll to interfac.dll.

The Machine Option dialog box has four tabs for the Zeiss interface:

PH9 tab

See the "Setting the Communication Protocol" topic. Default value is Comm Port 1, 9600 Baud, Even parity,8 data bits, and 2 stop bit.

Axis tab

See the "Assigning the Machine Axes" topic.

Debug tab

See the "Generating a Debug File" topic.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).