## Defining Probe Changers

To begin using your probe changer, you must first define the changer's port locations through the following probe changer calibration procedure. While PC-DMIS supports a variety of probe changers, only some of the calibration processes are discussed here. If you have a different probe changer type, different from the ones discussed, use the FCR25 one as a guide, as it should be similar enough for all supported types.

To begin this calibration process, you need to access the Probe Changer dialog box. Select Edit | Preferences | Probe Changer. At any time, you can view the information in the "Setting Up Probe Changer Options" topic of the "Setting Your Preferences" section to assist you in defining probe changers.

Terminology Note: While the Probe Changer dialog box uses the term "slot" instead of "port", the calibration prompts you will receive use the term "port". For this reason, this documentation will use the term "port" except when referring to Probe Changer dialog box items that use the term "slot".

More:

Calibrating the FCR25 Probe Changer

Calibrating the CW43 Probe Changer

Calibrating the SP600 Probe Changer

Calibrating the SCP600 Probe Changer

Calibrating the ACR1 Probe Changer

Showing an Animated Probe Changer