#### Leitz Protocol Setup tab

Machine Options dialog box - Leitz Protocol Setup tab

The Dea tab allows you to configure the following settings that are specific to the DEA interface:

Read Machine Defaults On Startup - When this check box is enabled, PC-DMIS will query the CMM's controller for the CMM defaults the next time you start PC-DMIS. The next time you run PC-DMIS, it will replace the values stored in the PC-DMIS Settings Editor with the CMM's original factory values stored in the controller. Note: This procedure does not restore original factory values if you have overwritten them on the controller's hard drive.

Use TCPIP link to drive Machine - Select this option if you are using TCP/IP to connect to your controller.

TCPIP Address - Specify the TCP/IP address for your machine controller - this is the IP address of the machine (CMM Controller) itself.

TCPIP Port Number - Specify the port number that the controller is configured to listen to. Typically this will be port 2001.

Terminal button - Clicking this will open a terminal session with you controller based on the TCPIP settings.

Disengage Drives - This check box should be selected for DCC machines which have drives that can be disengaged that are going to be used manually.

Compensation Type - Select from the following Volcomp methods: NONE, DEA Standard, DEA DLL (wcompens32), ASI, or Brown & Sharpe.

Compensation Mode - Select from the following compensation modes: Standard Machine, Dual Drive, Horizontal Arm (Arm 1), or Horizontal Arm (Arm 2).

Use DEA Structural Thermal Compensation OCX - Select this option to use DEA Structural Thermal Compensation OCX.

OCX Path - Specifies the path for the DEA Structural Thermal Compensation OCX file.

Machine Type - Specify the type of machine: Arm or Robot

Caution: These values should only be changed by a trained technician. Altering these values may give an undesired result.