#### Import a Unigraphics Part File

1. Select the File | Import menu option. The Import Data dialog box appears.

2. Select Unigraphics DCI from the List Files of Type list.

3. Navigate to the directory containing the UG file to import.

4. Select the UG part (with a .prt extension).

5. Click OK. This dialog box closes.

q If multiple coordinate systems are available, the DCI Coordinate System Select dialog box appears next, displaying a list of available coordinate systems.

DCI Coordinate System Select dialog box
Continue with step 6.

q If multiple coordinate systems aren't available, the DCI Coordinate System Select dialog box doesn't appear and you should skip to step 8.

6. Select a coordinate system to use as the base (or origin) for the CAD data as it is imported. The Absolute Coordinate System (ABS) is the default and uses the UG part's absolute coordinate system as the base. The Working Coordinate System (WCS) uses the current working coordinate system in the UG part as the base.

7. Click OK to accept the selected coordinate system. If you want to import the UG CAD data without a coordinate system, click the Cancel button instead.

8. PC-DMIS imports the selected file.

9. Use PC-DMIS as usual.