Current Help System: PC-DMIS Fixturing (View Core Help)

## Flexible Fixturing Setup in PC-DMIS

The Fixturing Setup dialog box (
Edit | Preferences | Fixturing or F12) allows you to define certain PC-DMIS specific parameters for your Flexible Fixturing system.

The initial setup of your Flexible Fixturing system is done through the Fixture Server Interface program (see ”r;Fixturing System Setup” section for more information on initial setup). To add or remove components of your Flexible Fixturing system, you must use the Fixture Server Interface program. The Fixturing Setup dialog box allows you to edit the parameters for components that were previously created.

Using the tabs available on this dialog box, you can:

- Specify the Volume Definition for each machine arm (Volume Definition tab).

- Define the location of the arm and arm gripper (Mount Points tab).

- Change your fixturing display options (Display Options tab)

- Define the Hole pattern for mounting columns (Hole Pattern Tab)

The Fixturing Setup button that is available from the Fixturing Setup dialog box will open the Fixturing System Setup dialog box. This dialog box is used in the initial setup of your fixturing system. For more information the ”r;Fixturing System Setup” section.

More:

Fixturing Setup: Volume Definition

Fixturing Setup: Mount Points

Fixturing Setup: Display Options

Fixturing Setup: Hole Pattern

Calibrating Fixture Columns