Current Help System: PC-DMIS Laser (View Core Help)

### Step 3: Define Setup Options for the Laser Sensor

1. If you see the Probe Utilities dialog box, close it down.

2. Open the Setup Options dialog box pressing the F5 key or select Edit | Preferences | Setup.

3. Select the Laser Sensor tab. This tab will vary, depending on the type of laser sensor that is specified in the port lock configuration. Specific information is provided for the following Probe Types:

- Perceptron Sensors

- Metris Sensors

- CMS Sensors

Registry Settings for Laser Probes

The Settings Editor has two settings that allow for the automated process of switching between a Contact probe and a Perceptron probe on a PH10 wrist (PICSDifferentialSwitchBit) and controlling the power on a laser probe warm up station (WarmUpStationPowerBit).

Next Step ...