Current Help System: PC-DMIS Laser (View Core Help)

#### Setting Boundary Points by Typing

To set the boundary of a scan by typing:

1. Double click the desired boundary point in the ‘#’ column. This will display the Edit Scan Item dialog box.

Edit Scan Item dialog box

2. Manually edit the X, Y or Z value.

3. Click the OK button to apply the changes.

The Cancel button disregards any changes that have been made and will close the dialog box.

The Next button accepts the changes and then brings up the next boundary point for editing.