NAME=CCD
Charge Coupled Device - This is one of the two main types of image sensors used in digital cameras.
NAME=Cloud of Points
The Cloud of Points command is a container for XYZ coordinate data. The data can be input from an external file, or it can come directly from a laser sensor through the referring scan command(s).
NAME=COP
The Cloud of Points command is a container for XYZ coordinate data. The data can be input from an external file, or it can come directly from a laser sensor through the referring scan command(s).
NAME=Exposure
This parameter controls the exposure of the Laser sensor.
NAME=Gauge side point
In a Flush and Gap Auto Feature, this is the point on the gauge surface side indicating where the flush should be measured. (also called the gauge point)
NAME=Master side point
In a Flush and Gap Auto Feature, this is the point on the master side surface wehre the flush is to be measured.
NAME=Overscan
This parameter controls how far beyond the nominal feature’s dimensions the probe will scan along both the major and minor axis of the feature.
NAME=Row Overlap
This parameter controls how far each pass will overlap with the previous pass.
NAME=Sensor Frequency
This parameter controls the internal sensor frequency of the probe. The value that is displayed is sensor pulses per second.
NAME=Surface CAD Model
A surface CAD model only has surfaces, and it does not create a solid. Some examples of this would be, a plane feature, or a cylinder surface where there is no closed volume.
