Current Help System: PC-DMIS Laser (View Core Help)

#### Setting Boundary Points Using the Read Position Method

To set the boundary of the scan using measured points,

1. Place the laser probe at the desired location.

2. Click the Probe Enable button on the jog box (only available on DEA/B&S machines).

Note: The probe enable light on the jog box will alternate off and on every time that it is pressed. This is not important and has no influence on the probe itself.

This automatically updates the value of the currently selected Boundary point in the Boundary Points and Vectors list. The focus moves to the next boundary point (if there are any in the list). In the case of a PATCH scan, an extra boundary point will be added automatically if the current point is the last point in the list. The PATCH scan will display the last point (this is the same as the previous point). PC-DMIS deletes this last point when you click the OK button.