Current Help System: PC-DMIS NC (View Core Help)

### Required Components for PC-DMIS NC

Below are the components you need in order to use PC-DMIS NC:

NC Machine with Probing - An NC machine with supported probing and probing macros installed.

Computer with PC-DMIS NC - A Computer running Windows XP 32-bit or Windows Vista 32-bit operating system. This computer must have the communication interfaces to accept data from the NC machine.

Communications Link - A communications link is required from the NC machine to the server computer running PC-DMIS NC or NCI. PC-DMIS NC version 1.0 currently supports serial, Ethernet, File, or HSSB interfaces to communicate between the two computers depending on the type of controller.

Controller Options -

- Fanuc: Macro B

- Fanuc: Macro memory expansion

- Siemens: HMI Advanced

- Heidenhain: LSV2

- Heidenhain: FCL3 Recommended for 3d probing

Port Lock - A hardware lock with the NC option programmed into it and licensed with the number of supported NC machines.

To enable this option, The port lock is programmed for the appropriate NC Interface:
• Fanuc machines with FOCAS option use the NCFanuc interface.
• Siemens machines with HMI Advanced option use the NCSiemens interface.