Current Help System: PC-DMIS NC (View Core Help)

#### Calibrate

- Probes - Supported for single and star tips. The controller resident probing macros may also be used in place of PC-DMIS NC generated calibration. Probe information (tool offset and effective ball diameter) will be requested from the control after every tool change operation. When PC-DMIS probe calibration is used, the probe length and effective ball diameter are managed by PC-DMIS. PC-DMIS NCI only uses PC-DMIS probe calibration.

- Rotary Table - Supported.