Current Help System: PC-DMIS NC (View Core Help)

### Step 1: Install the Probe and Macros

Use your probe system documentation to:

1. Install your probing system.

2. Install the probing macros.

Verify installation by calibrating the probe using the supplied calibration macros. If calibration macros are not supplied (i.e. Wilcox macros) run a calibration using PC-DMIS.

Note: Updates to the Renishaw macros have been made for optimum ball-center probing. If, prior to a probing cycle, your probe drops in the Z axis by the probe's diameter, contact Renishaw for an update.

Next Step...