Current Help System: PC-DMIS Portable (View Core Help)

### Tracker Status Bar

Tracker Status bar visibility can be toggled using the View | Statusbar | Tracker menu item.

Status Bar for 6dof Machines:

1. System Laser Status Indicator: This indicates the status of the Laser Tracker system.

- Green (Ready): The system is ready to measure

- Yellow (Busy): The system is currently measuring

- Red (Not ready): The system is not ready to measure. This may be due to a broken beam or a T-Probe reflector mismatch.

- Blue (6dof error): The camera cannot see enough LED’s on the device (usually T-Probe) to accurately calculate the orientation of the probe.

2. Active Station Indicator: Indicates which station is currently active. A double click onto the station Indicator opens the Station Manager dialog box.

- Red (Not oriented): The station position is not computed yet.

- Green (Oriented) The station position has been computed.

3. Environmental Parameter Display: Shows the active environmental parameters: temperature, pressure, and humidity. If no weather station is connected, it is possible to double-click on the edit boxes to change their values.

Status Bar for 3D Machines:

1. System Laser Status Indicator: This indicates the status of the Laser Tracker system.

1. - Green (Ready): The system is ready to measure

   - Yellow (Busy): The system is currently measuring

   - Red (Not ready): The system is not ready to measure. This may be due to a broken beam or a T-Probe reflector mismatch.

   - Blue (6dof error): The camera cannot see enough LED’s on the device (usually T-Probe) to accurately calculate the orientation of the probe.

2. Active Probe Name: This displays the currently active reflector.

3. Active Probe Diameter: Current reflector diameter.

4. Probe Compensation Indicator: Displays the current state of probe compensation.

5. Active Station Indicator: Indicates which station is currently active. A double click onto the station Indicator opens the Station Manager dialog box.

1. - Red (Not oriented): The station position is not computed yet.

   - Green (Oriented) The station position has been computed.

6. Environmental Parameter Display: Shows the active environmental parameters: temperature, pressure, and humidity. If no weather station is connected, it is possible to double-click on the edit boxes to change their values.

7. Power Lock Indicator: Displays the current status of PowerLock.

8. Battery Indicators: There are two indicators, one for the device and one for the controller. If the batteries are active, the status indicators display the percent power left in each individual battery. If the battery has more than 25% power, the background of the text is green. If the power level is between 10% & 25%, the color is yellow. If the power drops below 10%, the color changes to red. If the external power is active, the color of the fields change to gray and there are no numbers in the fields. Also, the battery icons change to display small external power chords.

   - Device Icons:

   - Controller Icons: