Current Help System: PC-DMIS Portable (View Core Help)

## Getting Started

There are a few basic steps that you should take to verify that your system has been properly prepared before beginning the measurement process with your portable arm.

If you plan to use a Perceptron Contour sensor with your Infinite arm, then you will also needs to follow the steps outlined in the "Configuring a Perceptron Contour Sensor" topic.

This section contains supplemental material to the standard WinRDS documentation for your Romer Infinite Arm. For additional setup information please consult the WinRDS documentation and Perceptron Contour sensor documentation.

To configure your Romer Infinite arm follow these steps:

- Step 1: Set Up the Romer Infinite Arm

- Step 2: Set WinRDS Environment Variables

- Step 3: Install PC-DMIS for Romer