Current Help System: PC-DMIS Settings Editor (View Core Help)

### Spacer

Use the DccSpacer value to affect this change rather then this value.

Defines the distance from the nominal point location that PC-DMIS will use to measure a plane if sample hits are specified.

Entry Name: Spacer

Entry Type: Real Number to specify distance. Default value is 0.

If no value is entered, PC-DMIS uses a default distance.