Current Help System: PC-DMIS Settings Editor (View Core Help)

### PTP_On Error

Allows you to define the default value for the On Error option that will be used when an Auto Feature is created. The On Error option allows improved error checking when PC-DMIS detects an unexpected or missed hit. When this option is set to TRUE, PC-DMIS automatically take a Read Position whenever an unexpected probe hit or missed probe hit takes place during the measurement cycle. This will also measure the entire feature with the new location obtained from the Read Position.

Entry Name: PTP_OnError

Entry Type: True/False value. Default value is FALSE.

Note: You can use this option on all the Auto Feature measurement types except Vector Point, Surface Point, Sphere, and High Point.

For additional information on what options you have when PC-DMIS detects unexpected or missed hits, see "Branching On a CMM Error" in the "Branching by Using Flow Control" section.