Current Help System: PC-DMIS Settings Editor (View Core Help)

### Flush and Gap CG Gray Sum Max

Provides the maximum pixel intensity beyond which pixels exceeding this value will not be used. This value is used when measuring laser flush a gap features using the Gray Sum locater type.

Entry Name: FlushAndGap_CGGraySumMax

Entry Type: Whole Number specifying maximum pixel intensity. Default value is 300.