Current Help System: PC-DMIS Settings Editor (View Core Help)

### CG Percentage

This value is used when the "SensorCGLocType" value is set to 0 (Brightest). See the "Laser Probe Toolbox: Laser Pixel Locator Properties tab" topic in the PC-DMIS Laser documentation for more information. The CG Percentage is the cutoff under which the data is discarded.

Entry Name: CGPercentage

Entry Type: Whole Number specifying percentage. Default value is 0.