Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision Optics Cal Focus Latency Fraction

Provides the optical zoom fraction at which the focus latency calibration will be executed. 0 is the maximum magnification and 1 is the minimum magnification.

Entry Name: ProbeQualVisionOpticsCalFocusLatencyFraction

Entry Type: Real Number specifying optical zoom fraction. The default is 0.5.