Current Help System: PC-DMIS Settings Editor (View Core Help)

### Colmap Up Tol

Provides the default Upper Tolerance value that is displayed in the Pointcloud Operator dialog box for a Point or Face Colormap operator.

Entry Name: ColmapUpTol

Entry Type: Real Number specifying upper tolerance. Default value is 1.

See the "FACE COLORMAP" or "POINT COLORMAP" topics of the PC-DMIS Laser help file for more information.