Current Help System: PC-DMIS Settings Editor (View Core Help)

### Scan Dialog Thick

Specifies the part thickness. PC-DMIS will apply this material thickness automatically when using CAD surface data. This thickness will be applied along the surface normal vector when FINDNOMS mode is selected and PC-DMIS pierces the CAD surfaces to get the nominals.

Entry Name: ScanDialogThick

Entry Type: Real Number specifying distance. Default value is 0.