Current Help System: PC-DMIS Settings Editor (View Core Help)

### Fixed Delta Scan Incr

Provides the distance that the probe will need to move before PC-DMIS takes a hit. This is the 3D distance between points. For example, if you use 5, and your units of measurement is millimeters, the probe has to move at least 5 mm from the last point before PC-DMIS accepts a hit from the controller.

Entry Name: FixedDeltaScanIncr

Entry Type: Real Number specifying distance. Default value is 0.1.