Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision Z Illum

Stores the default Z Illumination value that is used in the Measure Vision Probe dialog box. This illumination source will be used for the Z measurements. Normally, the top or ring for ring gage surface is used.

Entry Name: ProbeQualVisionZIllum

Entry Type: Real Number specifying illumination source value. The default is -1.