Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision Optics Cal Pixel Size Verify Tolerance

This sets the verification tolerance of the Pixel size verification. If the measured value differs from the nominal value by more than this tolerance, a <- symbol appears to the right of the error value in the Verification Complete dialog box.

Entry Name: ProbeQualVisionOpticsCalPixelSizeVerifyTolerance

Entry Type: Real Number specifying the tolerance value. The default is 1.0.