Current Help System: PC-DMIS Settings Editor (View Core Help)

### Sensor Exposure

Controls the exposure of the sensor. Values range from 0 to 15. Zero will work well for most parts, but parts which absorb a lot of light (such as a black anodized surface) may require that the value be set higher. Don’t set the value higher unless it is needed; doing so, may result in less accurate measurements.

Entry Name: SensorExposure

Entry Type: Real Number to specify an exposure value. Default value is 0.