Current Help System: PC-DMIS Settings Editor (View Core Help)

### UV Scan U End

Defines the end location of the area on the scan surface in the U direction (approximate X Direction) that will be included as part of the UV Scan. For example, a value of .9 would scan 90% of the way in the U direction.

Entry Name: UVScanUEnd

Entry Type: Real Number specifying portion of the whole surface. Default value is 0.9.