Current Help System: PC-DMIS Settings Editor (View Core Help)

### SP6MTX Entries for ANALOG_PROBING

You can only modify the SP6MTX entries using the PC-DMIS Settings Editor. These values were initially obtained when you completed the SP600 Lower Level Matrix calibration. PC-DMIS uses these values to create force variations needed to accurately obtain the low level matrix numbers for your probe.

For information on performing a lower level matrix calibration, see the "SP600 Calibration Procedures" topic in the "Defining Hardware" section in the main PC-DMIS help file.

More:

SP6MTX Lower Force

SP6MTXLowerForce_LSPX1C

SP6MTXLowerForce_LSPX1E

SP6MTXLowerForce_LSPX1M

SP6MTXLowerForce_LSPX1S

SP6MTXLowerForce_LSPX3

SP6MTXLowerForce_LSPX5

SP6MTXLowerForce_SP600

SP6MTXLowerForce_SP80

SP6MTX Max Force

SP6MTXMaxForce_LSPX1C

SP6MTXMaxForce_LSPX1E

SP6MTXMaxForce_LSPX1M

SP6MTXMaxForce_LSPX1S

SP6MTXMaxForce_LSPX3

SP6MTXMaxForce_LSPX5

SP6MTXMaxForce_SP600

SP6MTXMaxForce_SP80

SP6MTX Upper Force

SP6MTXUpperForce_LSPX1C

SP6MTXUpperForce_LSPX1E

SP6MTXUpperForce_LSPX1M

SP6MTXUpperForce_LSPX1S

SP6MTXUpperForce_LSPX3

SP6MTXUpperForce_LSPX5

SP6M TXUpperForce_SP600

SP6MTXUpperForce_SP80