Current Help System: PC-DMIS Settings Editor (View Core Help)

### Auto Change Stand Alone Delay

Represents the time in seconds that PC-DMIS will wait between positioning moves of the CMM for turning of the screw when dropping off or loading of a autojoint. You may have to experiment to get this setting correct. Usually values of between 2 to 5 seconds are adequate depending on the dip switch time delays and the change speed entered in the Probe Changer dialog box.

Entry Name: AutoChangeStandAloneDelay

Entry Type: Real Number to specify time in seconds. Default value is 3.