Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC XYZ_2

Provides the default "X" or "H" (height) value for the center location for all auto features except a line where it defines the start point. The value will represent Z value when the "Cartesian" value is set to TRUE (1), and H when it is set to FALSE (0). This value and the "DccXYZ_0" and "DccXYZ_1" values are used for Contact probes while the "Point1(XYZ)" values are used for Vision and Laser probes.

Entry Name: DccXYZ_2

Entry Type: Real Number to specify the Z or H value. Default value is 0.