Current Help System: PC-DMIS Settings Editor (View Core Help)

### Dual Arm Overlap

Determines the percentage of overlap to use which controls how the machine volume is divided between the two arms. At 0%, each arm would only be allowed to measure features that are within the half of the machine volume that is accessible to that arm. At 100%, Arm1 would be assigned to all the features.

Entry Name: DualArmOverlap

Entry Type: Real Number to specify a percentage. Default value is 100.