Current Help System: PC-DMIS Settings Editor (View Core Help)

### Allow Arbitrary Leitz Garage Placement

For some of the Leitz probe changer types, the first slot could be placed anywhere on the rack as desired, but subsequent slots had to be placed at specific distances along the rack relative to that first slot. In particular, the distance from the first slot to any other slot had to be an integer number of centimeters.

This entry determines whether or not you are allowed to position slots anywhere within the physical design of the rack and slot.

Entry Name: AllowArbitraryLeitzGaragePlacement

Entry Type: True/False value.

- If set to TRUE, you can position slots anywhere physically allowed by the rack and slot design. In some cases this may result in a small amount of additional motion during the probe change.

- If set to FALSE, you need to place the second and all subsequent slots at specified distances. Taking the time to carefully position the slots according to the spacing requirements may avoid the additional motion.