Current Help System: PC-DMIS Settings Editor (View Core Help)

### Scan Dialog Flush

Allows you to enter a flush thickness for the nominals if an edge hit is used and CAD data is available. This thickness is applied normal to the edge approach vector when finding the nominals for the scan. (This differs from the regular thickness which is applied along the surface normal.)

Entry Name: ScanDialogFlush

Entry Type: Real Number specifying distance. Default value is 0.1.