Current Help System: PC-DMIS Vision (View Core Help)

#### Measuring a Vector Point with NC-100

PC-DMIS allows several methods for measuring a vector point using the auto feature option. They are listed below:

Using Keyed in Data

This method allows you to key in the desired X, Y, Z, I, J, K values for the vector point.

Using Surface Data on the Screen

To generate a vector point using surface data:

1. Position the cursor in the Graphics Display window to indicate the desired location of the point (on the surface)

2. Click on the surface. PC-DMIS will highlight the selected surface.

3. Verify that the correct surface has been selected.

For complete information on this procedure, see "Using Surface Data on the Screen for a Vector Point" in the "Creating Auto Features" section.

Using Wire frame Data on the Screen

This is covered in "Using Wire frame Data on the Screen for a Vector Point" in the "Creating Auto Features" section.

Note: The mouse cannot be used in the Graphics Display window if CAD data is unavailable.