Current Help System: PC-DMIS Vision (View Core Help)

#### Vector Point with NC-100

NC-100 Vector Point Auto Feature

The Vector Point measurement option allows you to define a nominal point location as well as the nominal approach direction that the CMM will use to measure the point.

Single point measurement

To access the Vector Point option,

1. Access the Auto Features dialog box (
   Insert | Feature | Auto | Point | Vector).

2. Select the Vector Point auto feature type.

The Edit window command line for a sample Vector Point would read:

F_ID=AUTO/VECTOR POINT, THEO_THICKNESS = n, TOG , SNAP = Y/N
THEO/ TX,TY,TZ,TI,TJ,TK
ACTL/ X,Y,Z,I,J,K
TARG/ targX,targY,targZ,targI,targJ,targK
AUTO MOVE = Y/N, DISTANCE = n

More:

Vector Point Field Definitions with NC-100

Measuring a Vector Point with NC-100