Current Help System: PC-DMIS Vision (View Core Help)

#### Edge Point Type Definition with NC-100

EDGE NORMAL = This is the Normal edge type measurement that occurs at the surface height of the edge.

EDGE DELTAZ = This request allows the measurement of an edge at a specified depth in respect to the plane on which the surface lies.
Edge at a predefined depth from the part surface

EDGE HIGH = This request allows the measure of an edge at the maximum value in a specified direction.
Edge at maximum value along a known direction

EDGE BIGHOLE = This request allows the measure of an edge used to measure a part of a hole bigger than the sensor field of view.
Big hole contour measurement