Current Help System: PC-DMIS Vision (View Core Help)

#### Vision Field Definitions

The Edit window command line for a sample vision circle reads:

feature_name=FEAT/VISION/TOG1,TOG2,TOG3,TOG4
THEO/ <x_cord,y_cord,z_cord>,<i_vec,j_vec,k_vec>,diam
ACTL/ <x_cord,y_cord,z_cord>,<i_vec,j_vec,k_vec>,diam
TARG/ <x_cord,y_cord,z_cord>,<i_vec,j_vec,k_vec>
SHOW FEATURE PARAMETERS=TOG5

SURFACE=TOG6,n,EDGE/TOG6,n
MEASURE MODE=TOG7
RMEAS=CIR1,CIR1,CIR1
GRAPHICAL ANALYSIS=TOG8,n1,n2,n3
DIAGNOSTICS=TOG9
FEATURE LOCATOR=TOG10,n1,TOG11,n2,n3

SHOW VISION PARAMETERS=TOG12

TYPE=TOG13
COVERAGE=TOG14
MAGNIFICATION=0.843
HIT TARGET COLOR=TOG15,NOMINAL COLOR=TOG15
HIT TARGET/EA1,0.202,TOG16
FILTER=TOG17,n1,TOG18,n2,n3
EDGE=TOG19,n1,n2,n3,n4
FOCUS/TOG20,n1,n2,TOG21,TOG22

THEO, ACTL, and TARG values will vary depending on the feature type.

- THEO: Defines the theoretical values for measuring the Vision Auto Feature.

- ACTL: Defines the actual measured values of the measured Vision Auto Feature.

- TARG: Defines the target position for the measurement. Use these values when the THEO positions don't match the part. You should leave the THEO values to match the CAD positions, and results will be dimensioned to these values, but change the TARG values so that the feature will actually be measured in a slightly different place.