#### High Point Execution Example

- PC-DMIS will begin its search at the start point.

- It will take eight sampling hits around the start point at the distance specified in the Increment value.

- If a higher point is found, it becomes the new start point, and PC-DMIS again takes the eight sampling hits around the point. This continues until a higher point cannot be found at the increment distance.

- PC-DMIS then continues taking sampling hits reducing the increment value until the it matches the tolerance value thus completing the high point search.

- Once the search finishes, PC-DMIS displays the new high point value on the CAD model itself by moving the point ID to the found high point location within the search region.