#### Axis Basic Scan - Key In Method

This method lets you type the X, Y, and Z values of the start and end points for the Axis scan.

1. Click on the desired point in the List Box in the ‘#’ column. This will display an Edit Scan Item dialog box. The title bar of the dialog box displays the ID of the specific parameter being edited.

Edit Scan Item dialog box

2. Manually edit the X, Y, or Z value.

3. Click the OK button to apply the changes.

The Cancel button will disregard any changes that have been made and will close the dialog box.

You should also type the CutVec and the InitVec values of the axis using this same process.