#### Measure a Line

Red Dots show Possible Hit Locations

To measure a line, take two hits on side surface of the part just below the edge, the first hit on the left side of the part and the second hit to the right of the first hit. The direction is very important when measuring features, as PC-DMIS uses this information to create the coordinate axis system. Press the END key after the second hit. PC-DMIS will display a feature ID and measured line in the Graphics Display window.