### Step 9: Measure Additional Features

Use the probe to measure these three additional circles in the order indicated (item 1 as CIR2, item 2 as CIR3, and item 3 as CIR4):

And then a cone:

To measure a cone it is best to take 3 hits on the upper level and three hits on a lower level as shown in the drawing below.

Cone constructed from measurements at different depths

Note: For 3D measured features (Torus, Cylinder, Sphere, Cone) and for the 2D Plane feature, PC-DMIS will draw the feature with a shaded surface.

Go to the next step: "Construct New Features from Existing Features".