#### Tips to Use if None Explicitly Selected

This area lets you determine the action that PC-DMIS should take if you did not explicitly select any probe tips from the Active Tip List in the Probe Utilities dialog box prior to starting calibration. Note that if you explicitly choose tips from the Probe Utilities dialog box, only the selected tips will be used.

- If you choose the All option, PC-DMIS will use all existing probe tip angles in the current probe file.

- If you choose the Used In Program option, PC-DMIS will only use those probe tip angles that are used in the current part program for the current probe file. Note the following restrictions:

- This option may not achieve the desired result if you use it in a part program that has the Automatically Adjust Probe Head Wrist option enabled because the tips used in the program at the time of the calibration may change later as a result of the actual part alignment.

- This option only looks at the currently open part program. It does NOT try to look through references to external files such as subroutines.

- If you choose the Abort execution option, PC-DMIS will abort the execution or measurement, treating the condition of no tip angles selected as an error condition.

These options do not apply to all operation types and/or all hardware types. Its main purpose is to be used with the “Calibrate Tips” or “Qualification Check” operations when used with a fixed head, indexing wrist, or infinite wrist if used in an indexing (non-mapped) mode.