### Supported Interfaces

Not all interfaces support the ON ERROR command. Consult the following table to see if your interface is supported.

- If your interface is listed, a small black box indicates what error type is supported by that interface.

- If your interface isn't listed, then it's not able to use the ON ERROR command.

Supported Interfaces | Unexpected Probe Hit | Missed Probe Hit | Reflector Not Found
B&S Standard | ■ | ■ |
Dea |  | ■ |
Elm | ■ | ■ |
Federal/Renault | ■ | ■ |
Johansson | ■ | ■ |
Leica Tracker |  |  | ■
Leitz | ■ | ■ |
LK Direct (also known as LKRS232) | ■ | ■ |
LK Driver | ■ | ■ |
Metrolog | ■ | ■ |
Mitutoyo Bright | ■ | ■ |
Mitutoyo | ■ | ■ |
Mora | ■ | ■ |
Omnitech | ■ | ■ |
Renishaw | ■ | ■ |
Sharpe | ■ | ■ |
Sheffield | ■ | ■ |
Wenzel | ■ | ■ |
Zeiss | ■ | ■ |