### Constructing an Alignment Line

A line can be constructed through the current origin, normal to the current work plane. (Input features do not need to be provided.)

To Construct an Alignment Line:

1. Access the Construct Line dialog box (Insert | Feature | Constructed | Line).

2. Select the Alignment option.

3. Do not enter any features.

4. Click the Create button.

The Edit window command line for this option would read:
CONSTR/LINE,ALIGN,length

Constructing a Line Normal to the Work Plane | A - Line through the current origin normal to the current work plane. B - Current work plane. C - Origin