## Qualification Check

Type of Operation area showing Qualification Check option

After you calibrate the unit, a qualification check is recommended, but not required. Performing a qualification check will provide you with information regarding the general accuracy of the wrist calibration and future measurements. A qualification check can also be used to check the errors of new tips added to new probe files.

To perform a qualification check:

1. Access the Probe Utilities dialog box by selecting the Insert | Hardware Definition | Probe menu option.

2. Select the angles you wish to use for the qualification check from the Active Tip List. It’s recommended that you select probe angles both used and not used in the wrist calibration.

3. Click the Measure button. The Measure Probe dialog box appears.

4. Provide the parameters you wish to use during the calibration check including selecting the appropriate calibration tool.

5. Select the Qualification Check option from the Type of Operation area.

6. Click the Measure button.

7. Follow any on-screen instructions.