## Setting up a Multiple Arm CMM

To setup a multiple arm CMM, follow these steps:

More:

Step 1: Install PC-DMIS on All Computers

Step 2: Determine the Arm1 System

Step 3: Match the CMM Axes for Each Arm

Step 4: Configure Probe Head Mount Orientation

Step 5: Setup the Multiple Arm Connection

Step 6: Connect the Computers

Step 7: Enter Multiple Arm Mode

Step 8: Calibrate the Multiple Arm System

Step 9: Calibrate the Multiple Arm Probe Files

Step 10: Set the Multiple Arm Origin