#### Temperature Compensation Enabled

The Temperature Compensation Enabled check box tells PC-DMIS to use temperature compensation.

- If not selected, PC-DMIS does not perform any temperature compensation, and the TEMPCOMP command (if present in the part program) will have no effect.

- If selected, PC-DMIS behaves according to the input parameters.

Note: If you mark this check box and choose one of the compensation methods where PC-DMIS does the part compensation rather than the machine controller, the diameter for probes on non-portable machines in the Edit Probe Data dialog box may vary with the current part temperature. See "Edit Probe Data" in the "Defining Hardware" chapter.