### Default (I,J,K, Z) RMEAS Mode

When an Auto Feature has a relative planar measure feature associated with it (see "Relative Measurement area"), PC-DMIS measures the Auto Feature in a location that is adjusted according to the following rules:

- The measuring orientation of the Auto Feature is corrected by the same rotation offset that exists between the orientation of the nominal and the actual RMEAS feature.

- The measuring location of the Auto Feature is corrected by the same positional offset that exists between the location of the nominal and the actual RMEAS feature.

Suggestion from Brian Gudauskas: When an Auto Feature has a relative measure feature associated with it (see "Relative Measurement area"), PC-DMIS measures the Auto Feature in a location that is adjusted by the deviation of the relative feature.

Example: Suppose you measured a plane (PLN), and an Auto Circle (CIR1) referenced the plane as its RMEAS feature. When you measure CIR1 PC-DMIS will measure it in the referenced plane (PLN). See "Math Process of the Default RMEAS Mode:".

The Edit window command for this option reads:

RMEAS/DEFAULT (I,J,K, Z)

This is the default and usual RMEAS mode for sheet metal features.

More:

Math Process of the Default (I,J,K, Z) RMEAS Mode: