#### Continue

The Continue command button allows you to resume execution of a part program halted by a CMM motion error, or the Stop button. PC-DMIS allows you to select the specific location within the current feature where the probe is to resume measuring the part. The default location is displayed in the Machine Commands list. To select another location, simply pull down the drop-down arrow and select the desired line. PC-DMIS will continue the measurement process at the displayed location when the Continue button is pressed.