#### Step 6 - Measuring Port 1/PA25-SH Insert

You will be prompted through the process of measuring Port 1 (left-most port) through a series of message boxes. Follow the prompts and take the needed hits as shown in the pictures for each hit.

Hit 1 on Top surface

PC-DMIS MESSAGE: Please take a hit on the top face of the front left corner for port 1 (which is local port 1 on FCR25 unit number 1).

Using your machine's jog box, measure the first hit on the top surface of Port 1 as shown in the image to the right. When you click OK you will be prompted to take the hit with the Execution Mode Options dialog box. |

Hit 2 on Front surface

PC-DMIS MESSAGE: Please take a hit on the front face of the front left corner for port 1 (which is local port 1 on FCR25 unit number 1).

Using your machine jog box, measure the second hit on the front surface of Port 1 as shown in the image to the right. When you click OK you will be prompted to take the hit with the Execution Mode Options dialog box. |

Hit 3 on Inside surface

PC-DMIS MESSAGE: Please take a hit on the inside face of the front left corner for port 1 (which is local port 1 on FCR25 unit number 1).

Using your machine's jog box, measure the third hit on the inside surface of Port 1 as shown in the image to the right. When you click OK you will be prompted to take the hit with the Execution Mode Options dialog box. |

This set of three hits establishes the location for the tool changer. These three hits would be the same if the port didn't have an insert. If you used a PA25-20 insert in this port, the hits would be taken on the insert in a similar fashion.

You will now be asked to complete a few steps via the following dialog box.

PC-DMIS MESSAGE: Please do the following steps in the indicated order.

1. Remove the current SH-1/2/3 stylus.

2. Attach the SHSP (Stylus Holder Setting Piece).

3. Jog the probe to a safe location with a clear line of approach to the port(s) being calibrated.

4. Then click OK.

After you click OK the machine will begin DCC measurement.

Complete the instructions in the message box and remove the specified stylus (in this case the SH-1/2/3 stylus) and attach the SHSP as shown in the image to the right. Note: Whenever the instructions direct that you should jog the probe to a "safe location" or a location "with a clear line of approach" you should move the probe to a position that is in front of and slightly above the rack.

When you have completed these steps, Click OK and DCC measurement will begin.

PC-DMIS will automatically measure the three hits with the SHSP that were previously taken with the SH-1/2/3 stylus. It will also take a hit on the opposite inside face. This completes the measurement of Port 1.

In the next step, PC-DMIS will measure Port 3.

Next Step